**Nuclear Data Section**

**International Atomic Energy Agency**

**P.O.Box 100, A-1400 Vienna, Austria**

**Memo CP-D/991**

**Date:** 4 March 2020

**To:** Distribution

**From:** N. Otsuka

**Subject: Partial elastic scattering? (REACTION SF3=EL and SF5=\*PAR\*)**

Suspicious combination of SF3=EL and SF5=PAR in a REACTION code was found in 53 subentries. I checked each case against the source article and summarized proposed corrections as appended to this memo.

In 10256.004-005 and 40934.046-072, neutron strength functions are coded not only with L but also with J, and this could be a reason why the quantity has been expressed with SF5=PAR.

The following new data heading is proposed for update of O2232.002.

**Dictionary 24 (Data headings)**

E-EXC-C-ER (Error in excitation energy of initial compound nucleus)

**Distribution:**

[a.koning@iaea.org](mailto:a.koning@iaea.org)

[abhihere@gmail.com](mailto:abhihere@gmail.com)

[aloks279@gmail.com](mailto:aloks279@gmail.com)

daniela.foligno@oecd-nea.org

[dbrown@bnl.gov](mailto:dbrown@bnl.gov)

[draj@barc.gov.in](mailto:draj@barc.gov.in)

[fukahori.tokio@jaea.go.jp](mailto:fukahori.tokio@jaea.go.jp)

[ganesan555@gmail.com](mailto:ganesan555@gmail.com)

[gezg@ciae.ac.cn](mailto:gezg@ciae.ac.cn)

[iwamoto.osamu@jaea.go.jp](mailto:iwamoto.osamu@jaea.go.jp)

[j.c.sublet@iaea.org](mailto:j.c.sublet@iaea.org)

[jmwang@ciae.ac.cn](mailto:jmwang@ciae.ac.cn)

[kaltchenko@kinr.kiev.ua](mailto:kaltchenko@kinr.kiev.ua)

[kenya.suyama@oecd-nea.org](mailto:kenya.suyama@oecd-nea.org)

[kimura.atsushi04@jaea.go.jp](mailto:kimura.atsushi04@jaea.go.jp)

[l.vrapcenjak@iaea.org](mailto:l.vrapcenjak@iaea.org)

[manuel.bossant@oecd-nea.org](mailto:manuel.bossant@oecd-nea.org)

[masaaki@nucl.sci.hokudai.ac.jp](mailto:masaaki@nucl.sci.hokudai.ac.jp)

[michael.fleming@oecd-nea.org](mailto:michael.fleming@oecd-nea.org)

[mmarina@ippe.ru](mailto:mmarina@ippe.ru)

[nicolas.soppera@oecd-nea.org](mailto:nicolas.soppera@oecd-nea.org)

[n.otsuka@iaea.org](mailto:n.otsuka@iaea.org)

[nrdc@jcprg.org](mailto:nrdc@jcprg.org)

[odsurenn@gmail.com](mailto:odsurenn@gmail.com)

[ogritzay@kinr.kiev.ua](mailto:ogritzay@kinr.kiev.ua)

[ogrudzevich@ippe.ru](mailto:ogrudzevich@ippe.ru)

[otto.schwerer@aon.at](mailto:otto.schwerer@aon.at)

[pikulina@expd.vniief.ru](mailto:pikulina@expd.vniief.ru)

[pritychenko@bnl.gov](mailto:pritychenko@bnl.gov)

[s.okumura@iaea.org](mailto:s.okumura@iaea.org)

[samaev@obninsk.ru](mailto:samaev@obninsk.ru)

[sbabykina@yandex.ru](mailto:sbabykina@yandex.ru)

[scyang@kaeri.re.kr](mailto:scyang@kaeri.re.kr)

[selyankina@expd.vniief.ru](mailto:selyankina@expd.vniief.ru)

[sonzogni@bnl.gov](mailto:sonzogni@bnl.gov)

[stakacs@atomki.mta.hu](mailto:stakacs@atomki.mta.hu)

[stanislav.hlavac@savba.sk](mailto:stanislav.hlavac@savba.sk)

[sv.dunaeva@gmail.com](mailto:sv.dunaeva@gmail.com)

[tada@nucl.sci.hokudai.ac.jp](mailto:tada@nucl.sci.hokudai.ac.jp)

[taova@expd.vniief.ru](mailto:taova@expd.vniief.ru)

[tarkanyi@atomki.hu](mailto:tarkanyi@atomki.hu)

[vvvarlamov@gmail.com](mailto:vvvarlamov@gmail.com)

[v.zerkin@iaea.org](mailto:v.zerkin@iaea.org)

[vidyathakur@yahoo.co.in](mailto:vidyathakur@yahoo.co.in)

[vsemkova@inrne.bas.bg](mailto:vsemkova@inrne.bas.bg)

[yolee@kaeri.re.kr](mailto:yolee@kaeri.re.kr)

[zholdybayev@inp.kz](mailto:zholdybayev@inp.kz)

**Combination of SF3=EL and SF5=PAR in REACTION codes (EXFOR Master Ver. 2020-03-02)**

(All items are registered in the EXFOR Feedback List.)

|  |  |  |  |
| --- | --- | --- | --- |
| **EXFOR #** | **REACTION** | **Proposed corrections** | **Remark** |
| 10256.004 | (60-ND-145(N,EL),PAR,STF) | Delete SF5=PAR. SF1 must be 60-ND-143. | J dependent S0. |
| 10256.005 | (60-ND-145(N,EL),PAR,STF) | Delete SF5=PAR. | J dependent S0. |
| 12373.008 | ((92-U-235(N,EL)92-U-235,PAR,SIG)+ (92-U-235(N,INL)92-U-235,PAR,SIG)) | SF3 must be SCT. |  |
| 12844.002 | (26-FE-54(N,EL)26-FE-54,PAR,POL/DA,,ANA) | Delete SF5=PAR and E-LVL=0.0 MeV. |  |
| 12844.003 | (29-CU-65(N,EL)29-CU-65,PAR,POL/DA,,ANA) | Delete SF5=PAR and E-LVL=0.0 MeV. |  |
| 22052.004.2 | (82-PB-207(N,EL),PAR,WID/STR) | SF3 must be G. |  |
| 22052.004.3 | (82-PB-207(N,EL),PAR,WID/STR) | SF3 must be G. |  |
| 22773.004 | (3-LI-6(N,EL)3-LI-6,PAR,DA) | SF3 must be INL. |  |
| 23030.009 | 6-C-12(N,EL)6-C-12,PAR,KER | SF3 must be INL. |  |
| 40934.046 | 52-TE-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.047 | 51-SB-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.048 | 48-CD-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.049 | 47-AG-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.050 | 46-PD-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.051 | 45-RH-103(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.052 | 44-RU-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.053 | 42-MO-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.054 | 40-ZR-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.055 | 34-SE-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.056 | 32-GE-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.057 | 30-ZN-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.058 | 28-NI-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.059 | 26-FE-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.060 | 22-TI-0(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.061 | 48-CD-106(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.062 | 48-CD-108(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.063 | 48-CD-110(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.064 | 48-CD-112(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.065 | 48-CD-116(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.066 | 50-SN-116(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.067 | 50-SN-117(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.068 | 50-SN-118(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.069 | 50-SN-119(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.070 | 50-SN-120(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.071 | 50-SN-122(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 40934.072 | 50-SN-124(N,EL),PAR,STF | Delete SF5=PAR. | J dependent S1. |
| 41316.019 | (26-FE-56(N,G),PAR,WID)/ (26-FE-56(N,EL),PAR,WID) | ? | Not in the source article? |
| A0945.003.1 | (7-N-14(P,EL),PAR,WID) | ? | Question sent to Sergey Artemov. |
| A1431.007 | 3-LI-6(D,EL)3-LI-6,PAR,DA | Delete SF5=PAR and E-LVL=0.0 MeV. |  |
| A1431.008 | 3-LI-7(D,EL)3-LI-7,PAR,DA | Delete SF5=PAR and E-LVL=0.0 MeV. |  |
| A1432.009 | 4-BE-9(D,EL)4-BE-9,PAR,DA,,REL | Delete SF5=PAR and E-LVL=0.0 MeV. |  |
| C0075.002 | 12-MG-24(P,EL)12-MG-24,PAR,DA | Delete SF5=PAR and E-EXC=0. MeV in 001. | Treated as (p,p0) data in IBANDL. |
| C0075.003 | 12-MG-24(P,EL)12-MG-24,PAR,POL/DA,,ANA | Delete SF5=PAR and E-EXC=0. MeV in 001. |  |
| C0179.004 | 7-N-14(P,EL)7-N-14,PAR,SIG | Delete SF5=PAR. |  |
| C2269.002.1 | 16-S-31(P,G),PAR,WID | Delete SF5=PAR and E-LVL values. Add resonance energy. |  |
| C2269.002.2 | 16-S-31(P,EL),PAR,WID | Delete SF5=PAR and E-LVL values. Add resonance energy. |  |
| C2269.002.3 | 16-S-31(P,EL),PAR,WID/STR | Delete SF5=PAR and E-LVL values. Add resonance energy. |  |
| D0279.007 | 32-GE-74(3-LI-6,EL)32-GE-74,PAR,DA | SF3 must be INL. |  |
| D0294.003 | 12-MG-24(P,EL)12-MG-24,PAR,DA | SF3 must be INL. |  |
| F0655.004 | 14-SI-28(A,EL)14-SI-28,PAR,DA | SF3 must be INL. Add E-RSL=1 MeV (or E-CM -> E-CM-MIN/MAX) |  |
| F0722.003 | 5-B-11(HE3,EL)5-B-11,PAR,DA | Elastic and inelastic data sets must be separated to two subentries. |  |
| F1095.003 | 5-B-11(P,EL)5-B-11,PAR,DA,,RSD | SF3 must be INL. |  |
| O0192.002 | 82-PB-208(P,EL)82-PB-208,PAR,POL/DA | Delete SF5=PAR and E-LVL=0.00 MeV. |  |
| O1768.006 | 28-NI-64(A,EL)28-NI-64,PAR,DA | SF3 must be INL. |  |
| O1768.007 | 30-ZN-66(A,EL)30-ZN-66,PAR,DA | SF3 must be INL. |  |
| O2232.002 | 1-H-1(8-O-15,EL),PAR,WID | Delete SF5=PAR. E-LVL -> E-EXC-CMP; E-LVL-ERR -> E-EXC-C-ER | A new heading E-EXC-C-ER is proposed in this memo. |